# CONNECTION DETAILS OF RADIX 2 WIRE RH+T TRANSMITTER TYPE SC807 WITH DIGITAL METER TYPE RADIX X96A

## (1) Sensor Brown Colour Wire Connect to Digital Meter Terminal No.10

## (2) Sensor Blue Colour Wire Connect to Digital Meter Terminal No.14

## (3) Sensor Black Colour Wire Connect to Digital Meter Terminal No.34

## (4) Setting input 1 & 2 = 4 to 20 mAmp

## (5) Input 1 High = 100

## (6) Input 2 High = 50

 (Drawn By Mr. Adeeb Raza)